<h1><a id="_Toc438457861" name="_Toc438457861">Operation of the application</a></h1>

<h2><a id="_Toc438457862" name="_Toc438457862">Connect Controllers / Stations</a></h2>

<p class=MsoNormal>The first step is to look for the controllers and stations on the network. To do this, pull down the <b>Controllers / Stations</b> menu by clicking on the <img border=0 width=19 height=19 id="Imagen 73"
src="html/es/images/image015.jpg"> icon, then on the <img border=0 width=19 height=19 id="Imagen 74" src="html/es/images/image016.jpg"> icon to select the <b>Discover</b> option (This tool is only available for users that are administrators). This will carry out a search for all of the controllers that are connected to the network, showing them in a list to select the controllers to add. If controllers or stations have already been added, the <b>Resfresh</b> option can be used to update the status of the <b>Controllers / Stations</b> on the list.</p>

<p class=MsoNormal><span style='font-size:12.0pt;color:#4F81BD'>&nbsp;</span></p>

<h2><a id="_Toc438457863" name="_Toc438457863">Select a station</a></h2>

<p class=MsoNormal>The list of <b>Controllers / Stations</b> will show all of the controllers and stations that have been added to the application, showing: </p>

<p class=MsoListParagraphCxSpFirst style='margin-left:35.45pt;text-indent:-18.0pt'><span
style='font-family:Symbol'>· <span style='font:7.0pt "Times New Roman"'>&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;</span></span> A green icon <img border=0 width=20 height=19 id="Imagen 76"
src="html/es/images/image017.jpg"> if it is connected to the Web Manager application</p>

<p class=MsoListParagraphCxSpLast style='margin-left:35.45pt;text-indent:-18.0pt'><span
style='font-family:Symbol'>· <span style='font:7.0pt "Times New Roman"'>&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;</span></span> A red icon <img border=0 width=19 height=19 id="Imagen 79"
src="html/es/images/image018.jpg"> if there is currently no communication with the controller</p>

<p class=MsoNormal>If a controller is connected to the network and appears to be disconnected, the list can be updated using the Refresh option.</p>

<p class=MsoNormal>When a controller is selected, a menu drops down showing the different stations connected to it. When you click on a station, the application will show the working screen with the current status of the station.</p>

<p class=MsoNormal>&nbsp;</p>

<p class=MsoNormal align=center style='text-align:center'><img border=0 id="Imagen 80" src="html/es/images/image019.jpg"></p>

<h2><a id="_Toc438457864" name="_Toc438457864"><span lang=ES-TRAD>Station in Monitor Mode</span></a></h2>

<p class=MsoNormal>The connection with a <b>Station</b> is carried out by default in <b>Monitor Mode.</b> In this mode you can see the current operating parameters, the tools connected to the different ports and a graph of the temperature and / or power of each of the tools. Changing the operating parameters of the station is only possible in <b>Control Mode.</b> If the user's profile does not allow editing some of the station's parameters, the <b>Monitor Mode</b> icon will appear in grey.</p>

<p class=MsoNormal align=center style='text-align:center'><img border=0
width=76 height=22 id="Imagen 81"
src="html/es/images/image020.jpg">&nbsp;&nbsp;&nbsp;&nbsp; <img border=0 width=76
height=22 id="Imagen 82" src="html/es/images/image021.jpg">&nbsp;&nbsp;&nbsp;&nbsp; <img
border=0 width=76 height=20 id="Imagen 83"
src="html/es/images/image022.jpg"></p>

<p class=MsoNormal>For more information about the various parameters, see the station's manual that is available for free on JBC's website <a href="http://www.jbctools.com">www.jbctools.com</a></p>

<span style='font-size:9.0pt;font-family:"Verdana","sans-serif"'><br clear=all
style='page-break-before:always'></span>

<p class=MsoNormal align=left style='margin-bottom:0cm;margin-bottom:.0001pt;
text-align:left'><b><span style='font-size:12.0pt;color:#4F81BD'>&nbsp;</span></b></p>

<h2><a id="_Toc438457865" name="_Toc438457865">Station in Control Mode</a></h2>

<p class=MsoNormal>Once you have selected a station, an icon will appear at the top of the various menus in the shape of a padlock that shows the status of station as in <b>Control Mode.</b> If the icon is closed <img
border=0 width=19 height=19 id="Imagen 84"
src="html/es/images/image023.jpg"> that means that <b>Control Mode</b> is off, otherwise it appears open <img border=0 width=19 height=19
id="Imagen 85" src="html/es/images/image024.jpg"> . To enable or disable control, simply click on the icon. If the user's profile does not allow editing of some of the station's parameters, the <b>Monitor Mode</b> icon will appear in grey.</p>

<p class=MsoNormal align=center style='text-align:center'><img border=0
width=76 height=22 id="Imagen 86"
src="html/es/images/image020.jpg">&nbsp;&nbsp;&nbsp;&nbsp; <img border=0 width=76
height=22 id="Imagen 87" src="html/es/images/image025.jpg">&nbsp;&nbsp;&nbsp;&nbsp; <img
border=0 width=76 height=20 id="Imagen 88"
src="html/es/images/image022.jpg"></p>

<p class=MsoNormal>For more information about the various parameters, see the manual for RemoteManager that is available for free on JBC's website <a href="http://www.jbctools.com">www.jbctools.com</a></p>

<p class=MsoNormal>&nbsp;</p>

<p class=MsoNormal>&nbsp;</p>